IFC building model
Schema: "IFC2X3"
Description: "ViewDefinition[CoordinationView]"
Time stamp: "2016-04-27T11:17:19"
Author: "NBS"
Preprocessor: "Xbim.Ifc File Processor version 2.4.1.0"
Originating system: "Xbim version 2.4.1.0"
Authorization: "Add company name here"
Application: "Add company name here" version "0.2" identifier "Xbim Layered Material Converter" by Organization "NBS"

People and organizations
  Person "NBS" of Organization "Add company name here"
  Owner history of Person "NBS" of Organization "Add company name here" | application "Add company name here" version "0.2" identifier "Xbim Layered Material Converter" by Organization "NBS" | change ADDED | created 1461752239 (2016-04-27T10:17:19Z)
  Owner history of Person "NBS" of Organization "Add company name here" | application "Add company name here" version "0.2" identifier "Xbim Layered Material Converter" by Organization "NBS" | change MODIFIED | created 1461752239 (2016-04-27T10:17:19Z)

Units
  LENGTHUNIT: MILLI METRE
  AREAUNIT: SQUARE_METRE
  VOLUMEUNIT: CUBIC_METRE
  SOLIDANGLEUNIT: STERADIAN
  PLANEANGLEUNIT: RADIAN
  MASSUNIT: GRAM
  TIMEUNIT: SECOND
  THERMODYNAMICTEMPERATUREUNIT: DEGREE_CELSIUS
  LUMINOUSINTENSITYUNIT: LUMEN

Spatial structure
IFCPROJECT "Add company name here"
  IFCSITE "Default site"
    IFCBUILDING "Default building"
      contains 3 elements
        1 x IFCSLAB | type IFCSLABTYPE "NBS_CupaPizarras_NatSlts_Quarry4_5" | ROOF | names: "NBS_CupaPizarras_NatSlts_Quarry4_5" | material: layers "NBS_CupaPizarras_NatSlts_Quarry4_5" ("NBS_CupaPizarras_NatSlts_Quarry4_5" 5.)
        1 x IFCSLAB | type IFCSLABTYPE "NBS_CupaPizarras_NatSlts_Quarry4_65" | ROOF | names: "NBS_CupaPizarras_NatSlts_Quarry4_65" | material: layers "NBS_CupaPizarras_NatSlts_Quarry4_65" ("NBS_CupaPizarras_NatSlts_Quarry4_65" 6.5)
        1 x IFCSLAB | type IFCSLABTYPE "NBS_CupaPizarras_NatSlts_Quarry4_75" | ROOF | names: "NBS_CupaPizarras_NatSlts_Quarry4_75" | material: layers "NBS_CupaPizarras_NatSlts_Quarry4_75" ("NBS_CupaPizarras_NatSlts_Quarry4_75" 7.5)

Types
  IFCSLABTYPE "NBS_CupaPizarras_NatSlts_Quarry4_5" | ROOF | 1 occurrence | material: layers "NBS_CupaPizarras_NatSlts_Quarry4_5" ("NBS_CupaPizarras_NatSlts_Quarry4_5" 5.) | property sets: xbim_MaterialFunctionAssignment, NBS_General, NBS_Data, Pset_CoveringCommon, IFC, COBie
  IFCSLABTYPE "NBS_CupaPizarras_NatSlts_Quarry4_65" | ROOF | 1 occurrence | material: layers "NBS_CupaPizarras_NatSlts_Quarry4_65" ("NBS_CupaPizarras_NatSlts_Quarry4_65" 6.5) | property sets: xbim_MaterialFunctionAssignment, NBS_General, NBS_Data, Pset_CoveringCommon, IFC, COBie
  IFCSLABTYPE "NBS_CupaPizarras_NatSlts_Quarry4_75" | ROOF | 1 occurrence | material: layers "NBS_CupaPizarras_NatSlts_Quarry4_75" ("NBS_CupaPizarras_NatSlts_Quarry4_75" 7.5) | property sets: xbim_MaterialFunctionAssignment, NBS_General, NBS_Data, Pset_CoveringCommon, IFC, COBie

Property sets
  xbim_MaterialFunctionAssignment | properties | on 3 type objects
    MaterialFunctionAssignment (ifcpropertytablevalue)
  NBS_General | properties | on 1 type object
    Author = "NBS" (IFCTEXT)
    BIMObjectName = "NBS_CupaPizarras_NaturalSlates_Quarry4_5" (IFCTEXT)
    ManufacturerName = "Cupa Pizarras" (IFCTEXT)
    ManufacturerURL = "www.cupapizarras.com/uk" (IFCTEXT)
    NBSCertification = "http://www.nationalbimlibrary.com/cert/rljhsvlr" (IFCTEXT)
    NBSDescription = "Natural slates" (IFCTEXT)
    NBSNote = "n/a" (IFCTEXT)
    NBSOfficeMasterTag = "n/a" (IFCTEXT)
    NBSReference = "45-80-90/394" (IFCTEXT)
    NBSTypeID = "n/a" (IFCTEXT)
    ProductInformation = "www.cupapizarras.com/uk/documentation" (IFCTEXT)
    Revision = "n/a" (IFCTEXT)
    Uniclass2 = "45-93-72/478" (IFCTEXT)
    Uniclass2015Description = "Natural slates" (IFCTEXT)
    Uniclass2015Reference = "Pr_25_93_72_56" (IFCTEXT)
    Uniclass2015Version = "Products v1.1" (IFCTEXT)
    Version = "1" (IFCTEXT)
  NBS_General | properties | on 1 type object
    Author = "NBS" (IFCTEXT)
    BIMObjectName = "NBS_CupaPizarras_NaturalSlates_Quarry4_6.5" (IFCTEXT)
    ManufacturerName = "Cupa Pizarras" (IFCTEXT)
    ManufacturerURL = "www.cupapizarras.com/uk" (IFCTEXT)
    NBSCertification = "http://www.nationalbimlibrary.com/cert/rljhsvlr" (IFCTEXT)
    NBSDescription = "Natural slates" (IFCTEXT)
    NBSNote = "n/a" (IFCTEXT)
    NBSOfficeMasterTag = "n/a" (IFCTEXT)
    NBSReference = "45-80-90/394" (IFCTEXT)
    NBSTypeID = "n/a" (IFCTEXT)
    ProductInformation = "www.cupapizarras.com/uk/documentation" (IFCTEXT)
    Revision = "n/a" (IFCTEXT)
    Uniclass2 = "45-93-72/478" (IFCTEXT)
    Uniclass2015Description = "Natural slates" (IFCTEXT)
    Uniclass2015Reference = "Pr_25_93_72_56" (IFCTEXT)
    Uniclass2015Version = "Products v1.1" (IFCTEXT)
    Version = "1" (IFCTEXT)
  NBS_General | properties | on 1 type object
    Author = "NBS" (IFCTEXT)
    BIMObjectName = "NBS_CupaPizarras_NaturalSlates_Quarry4_7.5" (IFCTEXT)
    ManufacturerName = "Cupa Pizarras" (IFCTEXT)
    ManufacturerURL = "www.cupapizarras.com/uk" (IFCTEXT)
    NBSCertification = "http://www.nationalbimlibrary.com/cert/rljhsvlr" (IFCTEXT)
    NBSDescription = "Natural slates" (IFCTEXT)
    NBSNote = "n/a" (IFCTEXT)
    NBSOfficeMasterTag = "n/a" (IFCTEXT)
    NBSReference = "45-80-90/394" (IFCTEXT)
    NBSTypeID = "n/a" (IFCTEXT)
    ProductInformation = "www.cupapizarras.com/uk/documentation" (IFCTEXT)
    Revision = "n/a" (IFCTEXT)
    Uniclass2 = "45-93-72/478" (IFCTEXT)
    Uniclass2015Description = "Natural slates" (IFCTEXT)
    Uniclass2015Reference = "Pr_25_93_72_56" (IFCTEXT)
    Uniclass2015Version = "Products v1.1" (IFCTEXT)
    Version = "1" (IFCTEXT)
  NBS_Data | properties | on 2 type objects
    CarbonateContent = "0.0039" (IFCTEXT)
    CharacteristicModulusOfRuptureLongitudinal = "53 Mpa" (IFCTEXT)
    CharacteristicModulusOfRuptureTransverse = "56 MPa" (IFCTEXT)
    DimensionalTolerances = "+/- 5mm" (IFCTEXT)
    FormatOptions = "Rectangular, Ogival, Bullnose" (IFCTEXT)
    FreezeThawResistance = "Fulfill < 0.4%" (IFCTEXT)
    MeanFailureLoadLongitudinal = "n/a" (IFCTEXT)
    MeanFailureLoadTransverse = "n/a" (IFCTEXT)
    NominalThicknessAndIndividualThicknessVariation = "+/- 25%" (IFCTEXT)
    NonCarbonateCarbonContentMaximum = "0.51% fullfil (< 2%)" (IFCTEXT)
    SizeOptions = "500x250" (IFCTEXT)
    SlateSizeLengthMinimum = "500" (IFCTEXT)
    SlateSizeWidthMinimum = "250" (IFCTEXT)
    SlateTypeSource = "Quarry Armadilla. Benuza (León) Spain, operating since 1968 (28,000 t/year)" (IFCTEXT)
    StandardsMethodsOfTest = "EN 12326" (IFCTEXT)
    StandardsProductSpecification = "BS 680-2 and [CE marked] EN 12326 (NF 228-02/01/01, ATG H517)" (IFCTEXT)
    Strength = "n/a" (IFCTEXT)
    SulfurDioxideExposureTest = "S1" (IFCTEXT)
    ThermalCycleTest = "T1" (IFCTEXT)
    Type = "n/a" (IFCTEXT)
    WaterAbsorption = "0.29% Code: W1 (< 0.4%)" (IFCTEXT)
  NBS_Data | properties | on 1 type object
    CarbonateContent = "0.0039" (IFCTEXT)
    CharacteristicModulusOfRuptureLongitudinal = "53 Mpa" (IFCTEXT)
    CharacteristicModulusOfRuptureTransverse = "56 MPa" (IFCTEXT)
    DimensionalTolerances = "+/- 5mm" (IFCTEXT)
    FormatOptions = "Rectangular, Ogival, Bullnose" (IFCTEXT)
    FreezeThawResistance = "Fulfill < 0.4%" (IFCTEXT)
    MeanFailureLoadLongitudinal = "n/a" (IFCTEXT)
    MeanFailureLoadTransverse = "n/a" (IFCTEXT)
    NominalThicknessAndIndividualThicknessVariation = "+/- 25%" (IFCTEXT)
    NonCarbonateCarbonContentMaximum = "0.51% fullfil (< 2%)" (IFCTEXT)
    SizeOptions = "300x200, 400x200, 400x250, 500x250" (IFCTEXT)
    SlateSizeLengthMinimum = "300" (IFCTEXT)
    SlateSizeWidthMinimum = "200" (IFCTEXT)
    SlateTypeSource = "Quarry Armadilla. Benuza (León) Spain, operating since 1968 (28,000 t/year)" (IFCTEXT)
    StandardsMethodsOfTest = "EN 12326" (IFCTEXT)
    StandardsProductSpecification = "BS 680-2 and [CE marked] EN 12326 (NF 228-02/01/01, ATG H517)" (IFCTEXT)
    Strength = "n/a" (IFCTEXT)
    SulfurDioxideExposureTest = "S1" (IFCTEXT)
    ThermalCycleTest = "T1" (IFCTEXT)
    Type = "n/a" (IFCTEXT)
    WaterAbsorption = "0.29% Code: W1 (< 0.4%)" (IFCTEXT)
  Pset_CoveringCommon | properties | on 1 type object
    AcousticRating = "n/a" (IFCTEXT)
    Combustible = FALSE (IFCBOOLEAN)
    Finish = "R Excellence, H, Natural" (IFCTEXT)
    FireRating = "n/a" (IFCTEXT)
    FlammabilityRating = "n/a" (IFCTEXT)
    FragilityRating = "n/a" (IFCTEXT)
    Material = "Slate" (IFCTEXT)
    Reference = "n/a" (IFCTEXT)
    SurfaceSpreadOfFlame = "n/a" (IFCTEXT)
    TotalThickness = 5. (IFCLENGTHMEASURE) [MILLI METRE]
  Pset_CoveringCommon | properties | on 1 type object
    AcousticRating = "n/a" (IFCTEXT)
    Combustible = FALSE (IFCBOOLEAN)
    Finish = "R Excellence, H, Natural" (IFCTEXT)
    FireRating = "n/a" (IFCTEXT)
    FlammabilityRating = "n/a" (IFCTEXT)
    FragilityRating = "n/a" (IFCTEXT)
    Material = "Slate" (IFCTEXT)
    Reference = "n/a" (IFCTEXT)
    SurfaceSpreadOfFlame = "n/a" (IFCTEXT)
    TotalThickness = 6.5 (IFCLENGTHMEASURE) [MILLI METRE]
  Pset_CoveringCommon | properties | on 1 type object
    AcousticRating = "n/a" (IFCTEXT)
    Combustible = FALSE (IFCBOOLEAN)
    Finish = "Heavy" (IFCTEXT)
    FireRating = "n/a" (IFCTEXT)
    FlammabilityRating = "n/a" (IFCTEXT)
    FragilityRating = "n/a" (IFCTEXT)
    Material = "Slate" (IFCTEXT)
    Reference = "n/a" (IFCTEXT)
    SurfaceSpreadOfFlame = "n/a" (IFCTEXT)
    TotalThickness = 7.5 (IFCLENGTHMEASURE) [MILLI METRE]
  IFC | properties | on 3 type objects
    IfcExportAs = "IfcCoveringType" (IFCTEXT)
    IfcExportType = "ROOFING" (IFCTEXT)
  COBie | properties | on 1 type object
    AccessibilityPerformance = "n/a" (IFCTEXT)
    AssetIdentifier = "n/a" (IFCTEXT)
    AssetType = "Fixed" (IFCTEXT)
    BarCode = "n/a" (IFCTEXT)
    Category = "Pr_25_93_72_56:Natural slates" (IFCTEXT)
    CodePerformance = "n/a" (IFCTEXT)
    Color = "Blue black" (IFCTEXT)
    Constituents = "n/a" (IFCTEXT)
    Description = "Non-carbonated slate formed by tectonic compression, blue black slate with thin laminations and a smooth surface" (IFCTEXT)
    DurationUnit = "year" (IFCTEXT)
    ExpectedLife = "100" (IFCTEXT)
    Features = "n/a" (IFCTEXT)
    Grade = "n/a" (IFCTEXT)
    InstallationDate = "1900-12-31T23:59:59" (IFCTEXT)
    Manufacturer = "uk.cupa@cupagroup.com" (IFCTEXT)
    ModelNumber = "n/a" (IFCTEXT)
    ModelReference = "Quarry 4 - 5.0" (IFCTEXT)
    Name = "NaturalSlates_Quarry4_5_CupaPizarras" (IFCTEXT)
    NominalHeight = 5. (IFCLENGTHMEASURE) [MILLI METRE]
    NominalLength = 500. (IFCLENGTHMEASURE) [MILLI METRE]
    NominalWidth = 250. (IFCLENGTHMEASURE) [MILLI METRE]
    ReplacementCost = "n/a" (IFCTEXT)
    SerialNumber = "n/a" (IFCTEXT)
    Shape = "Rectangular" (IFCTEXT)
    Size = "500 x 250" (IFCTEXT)
    SustainabilityPerformance = "DAPc‐Bre Fullfil" (IFCTEXT)
    TagNumber = "n/a" (IFCTEXT)
    WarrantyDescription = "500x250" (IFCTEXT)
    WarrantyDurationLabor = "n/a" (IFCTEXT)
    WarrantyDurationParts = "n/a" (IFCTEXT)
    WarrantyDurationUnit = "year" (IFCTEXT)
    WarrantyGuarantorLabor = "n/a" (IFCTEXT)
    WarrantyGuarantorParts = "n/a" (IFCTEXT)
    WarrantyStartDate = "1900-12-31T23:59:59" (IFCTEXT)
  COBie | properties | on 1 type object
    AccessibilityPerformance = "n/a" (IFCTEXT)
    AssetIdentifier = "n/a" (IFCTEXT)
    AssetType = "Fixed" (IFCTEXT)
    BarCode = "n/a" (IFCTEXT)
    Category = "Pr_25_93_72_56:Natural slates" (IFCTEXT)
    CodePerformance = "n/a" (IFCTEXT)
    Color = "Blue black" (IFCTEXT)
    Constituents = "n/a" (IFCTEXT)
    Description = "Non-carbonated slate formed by tectonic compression, blue black slate with thin laminations and a smooth surface" (IFCTEXT)
    DurationUnit = "year" (IFCTEXT)
    ExpectedLife = "100" (IFCTEXT)
    Features = "n/a" (IFCTEXT)
    Grade = "n/a" (IFCTEXT)
    InstallationDate = "1900-12-31T23:59:59" (IFCTEXT)
    Manufacturer = "uk.cupa@cupagroup.com" (IFCTEXT)
    ModelNumber = "n/a" (IFCTEXT)
    ModelReference = "Quarry 4 - 6.5" (IFCTEXT)
    Name = "NaturalSlates_Quarry4_6.5_CupaPizarras" (IFCTEXT)
    NominalHeight = 6.5 (IFCLENGTHMEASURE) [MILLI METRE]
    NominalLength = 500. (IFCLENGTHMEASURE) [MILLI METRE]
    NominalWidth = 250. (IFCLENGTHMEASURE) [MILLI METRE]
    ReplacementCost = "n/a" (IFCTEXT)
    SerialNumber = "n/a" (IFCTEXT)
    Shape = "Rectangular" (IFCTEXT)
    Size = "500 x 250" (IFCTEXT)
    SustainabilityPerformance = "DAPc‐Bre Fullfil" (IFCTEXT)
    TagNumber = "n/a" (IFCTEXT)
    WarrantyDescription = "500x250" (IFCTEXT)
    WarrantyDurationLabor = "n/a" (IFCTEXT)
    WarrantyDurationParts = "n/a" (IFCTEXT)
    WarrantyDurationUnit = "year" (IFCTEXT)
    WarrantyGuarantorLabor = "n/a" (IFCTEXT)
    WarrantyGuarantorParts = "n/a" (IFCTEXT)
    WarrantyStartDate = "1900-12-31T23:59:59" (IFCTEXT)
  COBie | properties | on 1 type object
    AccessibilityPerformance = "n/a" (IFCTEXT)
    AssetIdentifier = "n/a" (IFCTEXT)
    AssetType = "Fixed" (IFCTEXT)
    BarCode = "n/a" (IFCTEXT)
    Category = "Pr_25_93_72_56:Natural slates" (IFCTEXT)
    CodePerformance = "n/a" (IFCTEXT)
    Color = "Blue black" (IFCTEXT)
    Constituents = "n/a" (IFCTEXT)
    Description = "Non-carbonated slate formed by tectonic compression, blue black slate with thin laminations and a smooth surface" (IFCTEXT)
    DurationUnit = "year" (IFCTEXT)
    ExpectedLife = "100" (IFCTEXT)
    Features = "n/a" (IFCTEXT)
    Grade = "n/a" (IFCTEXT)
    InstallationDate = "1900-12-31T23:59:59" (IFCTEXT)
    Manufacturer = "uk.cupa@cupagroup.com" (IFCTEXT)
    ModelNumber = "n/a" (IFCTEXT)
    ModelReference = "Quarry 4 - 7.5" (IFCTEXT)
    Name = "NaturalSlates_Quarry4_7.5_CupaPizarras" (IFCTEXT)
    NominalHeight = 7.5 (IFCLENGTHMEASURE) [MILLI METRE]
    NominalLength = 500. (IFCLENGTHMEASURE) [MILLI METRE]
    NominalWidth = 250. (IFCLENGTHMEASURE) [MILLI METRE]
    ReplacementCost = "n/a" (IFCTEXT)
    SerialNumber = "n/a" (IFCTEXT)
    Shape = "Rectangular" (IFCTEXT)
    Size = "500 x 250" (IFCTEXT)
    SustainabilityPerformance = "DAPc‐Bre Fullfil" (IFCTEXT)
    TagNumber = "n/a" (IFCTEXT)
    WarrantyDescription = "300x200, 400x200, 400x250, 500x250" (IFCTEXT)
    WarrantyDurationLabor = "n/a" (IFCTEXT)
    WarrantyDurationParts = "n/a" (IFCTEXT)
    WarrantyDurationUnit = "year" (IFCTEXT)
    WarrantyGuarantorLabor = "n/a" (IFCTEXT)
    WarrantyGuarantorParts = "n/a" (IFCTEXT)
    WarrantyStartDate = "1900-12-31T23:59:59" (IFCTEXT)