IFC building model
Schema: "IFC2X3"
Description: "ViewDefinition[CoordinationView]"
Time stamp: "2015-04-16T11:13:47"
Author: "NBS"
Preprocessor: "Xbim.Ifc File Processor version 2.4.1.0"
Originating system: "Xbim version 2.4.1.0"
Authorization: "Add company name here"
Application: "Add company name here" version "0.2" identifier "Xbim Layered Material Converter" by Organization "NBS"

People and organizations
  Person "NBS" of Organization "Add company name here"
  Owner history of Person "NBS" of Organization "Add company name here" | application "Add company name here" version "0.2" identifier "Xbim Layered Material Converter" by Organization "NBS" | change ADDED | created 1429179228 (2015-04-16T10:13:48Z)
  Owner history of Person "NBS" of Organization "Add company name here" | application "Add company name here" version "0.2" identifier "Xbim Layered Material Converter" by Organization "NBS" | change MODIFIED | created 1429179228 (2015-04-16T10:13:48Z)

Units
  LENGTHUNIT: MILLI METRE
  AREAUNIT: SQUARE_METRE
  VOLUMEUNIT: CUBIC_METRE
  SOLIDANGLEUNIT: STERADIAN
  PLANEANGLEUNIT: RADIAN
  MASSUNIT: GRAM
  TIMEUNIT: SECOND
  THERMODYNAMICTEMPERATUREUNIT: DEGREE_CELSIUS
  LUMINOUSINTENSITYUNIT: LUMEN

Spatial structure
IFCPROJECT "Add company name here"
  IFCSITE "Default site"
    IFCBUILDING "Default building"
      contains 5 elements
        1 x IFCWALLSTANDARDCASE | type IFCWALLTYPE "NBS_FunderMax_CompactOrSolidGradeLaminatesHPL_MaxExteriorFQuality_TK-2140x1060mm" | names: "NBS_FunderMax_CompactOrSolidGradeLaminatesHPL_MaxExteriorFQuality_TK-2140x1060mm" | material: layers "NBS_FunderMax_CompactOrSolidGradeLaminatesHPL_MaxExteriorFQuality_TK-2140x1060mm" ("NBS_FunderMax_CompactOrSolidGradeLaminatesHPL_MaxExteriorFQuality_TK-2140x1060mm" 10.) | property sets: Pset_WallCommon
        1 x IFCWALLSTANDARDCASE | type IFCWALLTYPE "NBS_FunderMax_CompactOrSolidGradeLaminatesHPL_MaxExteriorFQuality_GR-2800x1300mm" | names: "NBS_FunderMax_CompactOrSolidGradeLaminatesHPL_MaxExteriorFQuality_GR-2800x1300mm" | material: layers "NBS_FunderMax_CompactOrSolidGradeLaminatesHPL_MaxExteriorFQuality_GR-2800x1300mm" ("NBS_FunderMax_CompactOrSolidGradeLaminatesHPL_MaxExteriorFQuality_GR-2800x1300mm" 10.) | property sets: Pset_WallCommon
        1 x IFCWALLSTANDARDCASE | type IFCWALLTYPE "NBS_FunderMax_CompactOrSolidGradeLaminatesHPL_MaxExteriorFQuality_SP-2800x1850mm" | names: "NBS_FunderMax_CompactOrSolidGradeLaminatesHPL_MaxExteriorFQuality_SP-2800x1850mm" | material: layers "NBS_FunderMax_CompactOrSolidGradeLaminatesHPL_MaxExteriorFQuality_SP-2800x1850mm" ("NBS_FunderMax_CompactOrSolidGradeLaminatesHPL_MaxExteriorFQuality_SP-2800x1850mm" 10.) | property sets: Pset_WallCommon
        1 x IFCWALLSTANDARDCASE | type IFCWALLTYPE "NBS_FunderMax_CompactOrSolidGradeLaminatesHPL_MaxExteriorFQuality_JU-4100x1300mm" | names: "NBS_FunderMax_CompactOrSolidGradeLaminatesHPL_MaxExteriorFQuality_JU-4100x1300mm" | material: layers "NBS_FunderMax_CompactOrSolidGradeLaminatesHPL_MaxExteriorFQuality_JU-4100x1300mm" ("NBS_FunderMax_CompactOrSolidGradeLaminatesHPL_MaxExteriorFQuality_JU-4100x1300mm" 10.) | property sets: Pset_WallCommon
        1 x IFCWALLSTANDARDCASE | type IFCWALLTYPE "NBS_FunderMax_CompactOrSolidGradeLaminatesHPL_MaxExteriorFQuality_XL-4100x1850mm" | names: "NBS_FunderMax_CompactOrSolidGradeLaminatesHPL_MaxExteriorFQuality_XL-4100x1850mm" | material: layers "NBS_FunderMax_CompactOrSolidGradeLaminatesHPL_MaxExteriorFQuality_XL-4100x1850mm" ("NBS_FunderMax_CompactOrSolidGradeLaminatesHPL_MaxExteriorFQuality_XL-4100x1850mm" 10.) | property sets: Pset_WallCommon

Types
  IFCWALLTYPE "NBS_FunderMax_CompactOrSolidGradeLaminatesHPL_MaxExteriorFQuality_TK-2140x1060mm" | STANDARD | 1 occurrence | material: layers "NBS_FunderMax_CompactOrSolidGradeLaminatesHPL_MaxExteriorFQuality_TK-2140x1060mm" ("NBS_FunderMax_CompactOrSolidGradeLaminatesHPL_MaxExteriorFQuality_TK-2140x1060mm" 10.) | property sets: NBS_General, NBS_Data, Pset_CoveringCommon, COBie
  IFCWALLTYPE "NBS_FunderMax_CompactOrSolidGradeLaminatesHPL_MaxExteriorFQuality_GR-2800x1300mm" | STANDARD | 1 occurrence | material: layers "NBS_FunderMax_CompactOrSolidGradeLaminatesHPL_MaxExteriorFQuality_GR-2800x1300mm" ("NBS_FunderMax_CompactOrSolidGradeLaminatesHPL_MaxExteriorFQuality_GR-2800x1300mm" 10.) | property sets: NBS_General, NBS_Data, Pset_CoveringCommon, IFC, COBie
  IFCWALLTYPE "NBS_FunderMax_CompactOrSolidGradeLaminatesHPL_MaxExteriorFQuality_SP-2800x1850mm" | STANDARD | 1 occurrence | material: layers "NBS_FunderMax_CompactOrSolidGradeLaminatesHPL_MaxExteriorFQuality_SP-2800x1850mm" ("NBS_FunderMax_CompactOrSolidGradeLaminatesHPL_MaxExteriorFQuality_SP-2800x1850mm" 10.) | property sets: NBS_General, NBS_Data, Pset_CoveringCommon, IFC, COBie
  IFCWALLTYPE "NBS_FunderMax_CompactOrSolidGradeLaminatesHPL_MaxExteriorFQuality_JU-4100x1300mm" | STANDARD | 1 occurrence | material: layers "NBS_FunderMax_CompactOrSolidGradeLaminatesHPL_MaxExteriorFQuality_JU-4100x1300mm" ("NBS_FunderMax_CompactOrSolidGradeLaminatesHPL_MaxExteriorFQuality_JU-4100x1300mm" 10.) | property sets: NBS_General, NBS_Data, Pset_CoveringCommon, IFC, COBie
  IFCWALLTYPE "NBS_FunderMax_CompactOrSolidGradeLaminatesHPL_MaxExteriorFQuality_XL-4100x1850mm" | STANDARD | 1 occurrence | material: layers "NBS_FunderMax_CompactOrSolidGradeLaminatesHPL_MaxExteriorFQuality_XL-4100x1850mm" ("NBS_FunderMax_CompactOrSolidGradeLaminatesHPL_MaxExteriorFQuality_XL-4100x1850mm" 10.) | property sets: NBS_General, NBS_Data, Pset_CoveringCommon, IFC, COBie

Property sets
  Pset_WallCommon | properties | on 5 objects (5 IFCWALLSTANDARDCASE)
    IsExternal = TRUE (IFCBOOLEAN)
  NBS_General | properties | on 1 type object
    Author = "NBS" (IFCTEXT)
    BIMObjectName = "NBS_FunderMax_CompactOrSolidGradeLaminatesHPL_MaxExteriorFQuality_TK-2800x1300mm" (IFCTEXT)
    ManufacturerName = "FunderMax GmbH" (IFCTEXT)
    ManufacturerURL = "www.fundermax.at/en.html" (IFCTEXT)
    NBSCertification = "www.nationalbimlibrary.com/cert/cgl3sa4r" (IFCTEXT)
    NBSDescription = "Compact or solid grade laminates (HPL)" (IFCTEXT)
    NBSNote = "n/a" (IFCTEXT)
    NBSOfficeMasterTag = "n/a" (IFCTEXT)
    NBSReference = "45-45-65/360" (IFCTEXT)
    NBSTypeID = "n/a" (IFCTEXT)
    ProductInformation = "www.fundermax.at/exterior/fassadenplatten/detail/max-exterior-f-qualitaet.html" (IFCTEXT)
    Revision = "n/a" (IFCTEXT)
    Uniclass2015Code = "Pr_25_71_63_15" (IFCTEXT)
    Uniclass2015Title = "Compact or solid grade high-pressure laminate (HPL) boards" (IFCTEXT)
    Uniclass2015Version = "Products v1.4" (IFCTEXT)
    Version = "2" (IFCTEXT)
  NBS_General | properties | on 1 type object
    Author = "NBS" (IFCTEXT)
    BIMObjectName = "NBS_FunderMax_CompactOrSolidGradeLaminatesHPL_MaxExteriorFQuality_GR-2800x1300mm" (IFCTEXT)
    ManufacturerName = "FunderMax GmbH" (IFCTEXT)
    ManufacturerURL = "www.fundermax.at/en.html" (IFCTEXT)
    NBSCertification = "www.nationalbimlibrary.com/cert/cgl3sa4r" (IFCTEXT)
    NBSDescription = "Compact or solid grade laminates (HPL)" (IFCTEXT)
    NBSNote = "n/a" (IFCTEXT)
    NBSOfficeMasterTag = "n/a" (IFCTEXT)
    NBSReference = "45-45-65/360" (IFCTEXT)
    NBSTypeID = "n/a" (IFCTEXT)
    ProductInformation = "www.fundermax.at/exterior/fassadenplatten/detail/max-exterior-f-qualitaet.html" (IFCTEXT)
    Revision = "n/a" (IFCTEXT)
    Uniclass2015Code = "Pr_25_71_63_15" (IFCTEXT)
    Uniclass2015Title = "Compact or solid grade high-pressure laminate (HPL) boards" (IFCTEXT)
    Uniclass2015Version = "Products v1.4" (IFCTEXT)
    Version = "2" (IFCTEXT)
  NBS_General | properties | on 1 type object
    Author = "NBS" (IFCTEXT)
    BIMObjectName = "NBS_FunderMax_CompactOrSolidGradeLaminatesHPL_MaxExteriorFQuality_SP-2800x1854mm" (IFCTEXT)
    ManufacturerName = "FunderMax GmbH" (IFCTEXT)
    ManufacturerURL = "www.fundermax.at/en.html" (IFCTEXT)
    NBSCertification = "www.nationalbimlibrary.com/cert/cgl3sa4r" (IFCTEXT)
    NBSDescription = "Compact or solid grade laminates (HPL)" (IFCTEXT)
    NBSNote = "n/a" (IFCTEXT)
    NBSOfficeMasterTag = "n/a" (IFCTEXT)
    NBSReference = "45-45-65/360" (IFCTEXT)
    NBSTypeID = "n/a" (IFCTEXT)
    ProductInformation = "www.fundermax.at/exterior/fassadenplatten/detail/max-exterior-f-qualitaet.html" (IFCTEXT)
    Revision = "n/a" (IFCTEXT)
    Uniclass2015Code = "Pr_25_71_63_15" (IFCTEXT)
    Uniclass2015Title = "Compact or solid grade high-pressure laminate (HPL) boards" (IFCTEXT)
    Uniclass2015Version = "Products v1.4" (IFCTEXT)
    Version = "2" (IFCTEXT)
  NBS_General | properties | on 1 type object
    Author = "NBS" (IFCTEXT)
    BIMObjectName = "NBS_FunderMax_CompactOrSolidGradeLaminatesHPL_MaxExteriorFQuality_JU-4100x1300mm" (IFCTEXT)
    ManufacturerName = "FunderMax GmbH" (IFCTEXT)
    ManufacturerURL = "www.fundermax.at/en.html" (IFCTEXT)
    NBSCertification = "www.nationalbimlibrary.com/cert/cgl3sa4r" (IFCTEXT)
    NBSDescription = "Compact or solid grade laminates (HPL)" (IFCTEXT)
    NBSNote = "n/a" (IFCTEXT)
    NBSOfficeMasterTag = "n/a" (IFCTEXT)
    NBSReference = "45-45-65/360" (IFCTEXT)
    NBSTypeID = "n/a" (IFCTEXT)
    ProductInformation = "www.fundermax.at/exterior/fassadenplatten/detail/max-exterior-f-qualitaet.html" (IFCTEXT)
    Revision = "n/a" (IFCTEXT)
    Uniclass2015Code = "Pr_25_71_63_15" (IFCTEXT)
    Uniclass2015Title = "Compact or solid grade high-pressure laminate (HPL) boards" (IFCTEXT)
    Uniclass2015Version = "Products v1.4" (IFCTEXT)
    Version = "2" (IFCTEXT)
  NBS_General | properties | on 1 type object
    Author = "NBS" (IFCTEXT)
    BIMObjectName = "NBS_FunderMax_CompactOrSolidGradeLaminatesHPL_MaxExteriorFQuality_XL-4100x1850mm" (IFCTEXT)
    ManufacturerName = "FunderMax GmbH" (IFCTEXT)
    ManufacturerURL = "www.fundermax.at/en.html" (IFCTEXT)
    NBSCertification = "www.nationalbimlibrary.com/cert/cgl3sa4r" (IFCTEXT)
    NBSDescription = "Compact or solid grade laminates (HPL)" (IFCTEXT)
    NBSNote = "n/a" (IFCTEXT)
    NBSOfficeMasterTag = "n/a" (IFCTEXT)
    NBSReference = "45-45-65/360" (IFCTEXT)
    NBSTypeID = "n/a" (IFCTEXT)
    ProductInformation = "www.fundermax.at/exterior/fassadenplatten/detail/max-exterior-f-qualitaet.html" (IFCTEXT)
    Revision = "n/a" (IFCTEXT)
    Uniclass2015Code = "Pr_25_71_63_15" (IFCTEXT)
    Uniclass2015Title = "Compact or solid grade high-pressure laminate (HPL) boards" (IFCTEXT)
    Uniclass2015Version = "Products v1.4" (IFCTEXT)
    Version = "2" (IFCTEXT)
  NBS_Data | properties | on 2 type objects
    ApparentDensity = "1.35 g/cm³" (IFCTEXT)
    Certification = "CE- marked, BBA 12/4937" (IFCTEXT)
    Core = "F-quality, colour brown" (IFCTEXT)
    Edges = "n/a" (IFCTEXT)
    FinishOptions = "NT, NH/NT, NG/NG, range of colours available" (IFCTEXT)
    FlexuralStrength = "≥ 90 MPa" (IFCTEXT)
    ModulusOfElasticity = "≥ 9.0 MPa" (IFCTEXT)
    PanelSizeLength = "2800 mm" (IFCTEXT)
    PanelSizeWidth = "1300 mm" (IFCTEXT)
    Specials = "n/a" (IFCTEXT)
    Surface = "NT" (IFCTEXT)
    TensileStrength = "≥ 80 MPa" (IFCTEXT)
    ThermalConductivity = "0.3 W/mK" (IFCTEXT)
    ThermalExpansionCoefficient = "18x10^-6 1/K" (IFCTEXT)
    ThicknessOptions = "2-15 mm" (IFCTEXT)
    Tolerances = "0-10 mm to BS EN 438-6" (IFCTEXT)
    UVResistance = "4-5" (IFCTEXT)
    WaterVapourDiffusionResistance = "17.200 μ" (IFCTEXT)
  NBS_Data | properties | on 1 type object
    ApparentDensity = "1.35 g/cm³" (IFCTEXT)
    Certification = "CE- marked, BBA 12/4937" (IFCTEXT)
    Core = "F-quality, colour brown" (IFCTEXT)
    Edges = "n/a" (IFCTEXT)
    FinishOptions = "NT, NH/NT, NG/NG, range of colours available" (IFCTEXT)
    FlexuralStrength = "≥ 90 MPa" (IFCTEXT)
    ModulusOfElasticity = "≥ 9.0 MPa" (IFCTEXT)
    PanelSizeLength = "2800 mm" (IFCTEXT)
    PanelSizeWidth = "1850 mm" (IFCTEXT)
    Specials = "n/a" (IFCTEXT)
    Surface = "NT" (IFCTEXT)
    TensileStrength = "≥ 80 MPa" (IFCTEXT)
    ThermalConductivity = "0.3 W/mK" (IFCTEXT)
    ThermalExpansionCoefficient = "18x10^-6 1/K" (IFCTEXT)
    ThicknessOptions = "2-15 mm" (IFCTEXT)
    Tolerances = "0-10 mm to BS EN 438-6" (IFCTEXT)
    UVResistance = "4-5" (IFCTEXT)
    WaterVapourDiffusionResistance = "17.200 μ" (IFCTEXT)
  NBS_Data | properties | on 1 type object
    ApparentDensity = "1.35 g/cm³" (IFCTEXT)
    Certification = "CE- marked, BBA 12/4937" (IFCTEXT)
    Core = "F-quality, colour brown" (IFCTEXT)
    Edges = "n/a" (IFCTEXT)
    FinishOptions = "NT, NH/NT, NG/NG, range of colours available" (IFCTEXT)
    FlexuralStrength = "≥ 90 MPa" (IFCTEXT)
    ModulusOfElasticity = "≥ 9.0 MPa" (IFCTEXT)
    PanelSizeLength = "4100 mm" (IFCTEXT)
    PanelSizeWidth = "1300 mm" (IFCTEXT)
    Specials = "n/a" (IFCTEXT)
    Surface = "NT" (IFCTEXT)
    TensileStrength = "≥ 80 MPa" (IFCTEXT)
    ThermalConductivity = "0.3 W/mK" (IFCTEXT)
    ThermalExpansionCoefficient = "18x10^-6 1/K" (IFCTEXT)
    ThicknessOptions = "2-15 mm" (IFCTEXT)
    Tolerances = "0-10 mm to BS EN 438-6" (IFCTEXT)
    UVResistance = "4-5" (IFCTEXT)
    WaterVapourDiffusionResistance = "17.200 μ" (IFCTEXT)
  NBS_Data | properties | on 1 type object
    ApparentDensity = "1.35 g/cm³" (IFCTEXT)
    Certification = "CE- marked, BBA 12/4937" (IFCTEXT)
    Core = "F-quality, colour brown" (IFCTEXT)
    Edges = "n/a" (IFCTEXT)
    FinishOptions = "NT, NH/NT, NG/NG, range of colours available" (IFCTEXT)
    FlexuralStrength = "≥ 90 MPa" (IFCTEXT)
    ModulusOfElasticity = "≥ 9.0 MPa" (IFCTEXT)
    PanelSizeLength = "4100 mm" (IFCTEXT)
    PanelSizeWidth = "1850 mm" (IFCTEXT)
    Specials = "n/a" (IFCTEXT)
    Surface = "NT" (IFCTEXT)
    TensileStrength = "≥ 80 MPa" (IFCTEXT)
    ThermalConductivity = "0.3 W/mK" (IFCTEXT)
    ThermalExpansionCoefficient = "18x10^-6 1/K" (IFCTEXT)
    ThicknessOptions = "2-15 mm" (IFCTEXT)
    Tolerances = "0-10 mm to BS EN 438-6" (IFCTEXT)
    UVResistance = "4-5" (IFCTEXT)
    WaterVapourDiffusionResistance = "17.200 μ" (IFCTEXT)
  Pset_CoveringCommon | properties | on 5 type objects
    AcousticRating = "n/a" (IFCTEXT)
    Combustible = FALSE (IFCBOOLEAN)
    Finish = "Acrylic PUR-resin" (IFCTEXT)
    FireRating = "Euroclass B-s2, d0" (IFCTEXT)
    FlammabilityRating = "n/a" (IFCTEXT)
    FragilityRating = "n/a" (IFCTEXT)
    IsExternal = TRUE (IFCBOOLEAN)
    Material = "Duromer HPL" (IFCTEXT)
    Reference = "n/a" (IFCTEXT)
    SurfaceSpreadOfFlame = "n/a" (IFCTEXT)
    TotalThickness = 10. (IFCLENGTHMEASURE) [MILLI METRE]
  COBie | properties | on 1 type object
    AccessibilityPerformance = "n/a" (IFCTEXT)
    AssetIdentifier = "n/a" (IFCTEXT)
    AssetType = "Fixed" (IFCTEXT)
    BarCode = "n/a" (IFCTEXT)
    Category = "Pr_25_71_63_15:Compact or solid grade high-pressure laminate (HPL) boards" (IFCTEXT)
    CodePerformance = "n/a" (IFCTEXT)
    Color = "n/a" (IFCTEXT)
    Constituents = "n/a" (IFCTEXT)
    Description = "Duromer high-pressure laminate panels (HPL) in accordance with BS EN 438-6 Type EDF, suitable for long-lasting balconies and façade claddings" (IFCTEXT)
    DurationUnit = "year" (IFCTEXT)
    ExpectedLife = "n/a" (IFCTEXT)
    Features = "Weather-resistant, flame-retardant core, lightfast, double-hardened, scratch and solvent resistant, easy to clean, custom shapes also available" (IFCTEXT)
    Grade = "To BS EN 438-6, Type EDF" (IFCTEXT)
    InstallationDate = "1900-12-31T23:59:59" (IFCTEXT)
    Manufacturer = "office@fundermax.biz" (IFCTEXT)
    ModelNumber = "n/a" (IFCTEXT)
    ModelReference = "Max Exterior F-Quality" (IFCTEXT)
    Name = "CompactOrSolidGradeLaminatesHPL_MaxExteriorFQuality_TK-2140x1060mm_FunderMax" (IFCTEXT)
    NominalHeight = 10. (IFCLENGTHMEASURE) [MILLI METRE]
    NominalLength = 2800. (IFCLENGTHMEASURE) [MILLI METRE]
    NominalWidth = 1300. (IFCLENGTHMEASURE) [MILLI METRE]
    ReplacementCost = "n/a" (IFCTEXT)
    SerialNumber = "n/a" (IFCTEXT)
    Shape = "Rectangle" (IFCTEXT)
    Size = "2800 x 1300 x 10 mm" (IFCTEXT)
    SustainabilityPerformance = "n/a" (IFCTEXT)
    TagNumber = "n/a" (IFCTEXT)
    WarrantyDescription = "n/a" (IFCTEXT)
    WarrantyDurationLabor = "n/a" (IFCTEXT)
    WarrantyDurationParts = "n/a" (IFCTEXT)
    WarrantyDurationUnit = "year" (IFCTEXT)
    WarrantyGuarantorLabor = "n/a" (IFCTEXT)
    WarrantyGuarantorParts = "n/a" (IFCTEXT)
    WarrantyStartDate = "1900-12-31T23:59:59" (IFCTEXT)
  COBie | properties | on 1 type object
    AccessibilityPerformance = "n/a" (IFCTEXT)
    AssetIdentifier = "n/a" (IFCTEXT)
    AssetType = "Fixed" (IFCTEXT)
    BarCode = "n/a" (IFCTEXT)
    Category = "Pr_25_71_63_15:Compact or solid grade high-pressure laminate (HPL) boards" (IFCTEXT)
    CodePerformance = "n/a" (IFCTEXT)
    Color = "n/a" (IFCTEXT)
    Constituents = "n/a" (IFCTEXT)
    Description = "Duromer high-pressure laminate panels (HPL) in accordance with BS EN 438-6 Type EDF, suitable for long-lasting balconies and façade claddings" (IFCTEXT)
    DurationUnit = "year" (IFCTEXT)
    ExpectedLife = "n/a" (IFCTEXT)
    Features = "Weather-resistant, flame-retardant core, lightfast, double-hardened, scratch and solvent resistant, easy to clean, custom shapes also available" (IFCTEXT)
    Grade = "To BS EN 438-6, Type EDF" (IFCTEXT)
    InstallationDate = "1900-12-31T23:59:59" (IFCTEXT)
    Manufacturer = "office@fundermax.biz" (IFCTEXT)
    ModelNumber = "n/a" (IFCTEXT)
    ModelReference = "Max Exterior F-Quality" (IFCTEXT)
    Name = "CompactOrSolidGradeLaminatesHPL_MaxExteriorFQuality_GR-2800x1300mm_FunderMax" (IFCTEXT)
    NominalHeight = 10. (IFCLENGTHMEASURE) [MILLI METRE]
    NominalLength = 2800. (IFCLENGTHMEASURE) [MILLI METRE]
    NominalWidth = 1300. (IFCLENGTHMEASURE) [MILLI METRE]
    ReplacementCost = "n/a" (IFCTEXT)
    SerialNumber = "n/a" (IFCTEXT)
    Shape = "Rectangle" (IFCTEXT)
    Size = "2800 x 1300 x 10 mm" (IFCTEXT)
    SustainabilityPerformance = "n/a" (IFCTEXT)
    TagNumber = "n/a" (IFCTEXT)
    WarrantyDescription = "n/a" (IFCTEXT)
    WarrantyDurationLabor = "n/a" (IFCTEXT)
    WarrantyDurationParts = "n/a" (IFCTEXT)
    WarrantyDurationUnit = "year" (IFCTEXT)
    WarrantyGuarantorLabor = "n/a" (IFCTEXT)
    WarrantyGuarantorParts = "n/a" (IFCTEXT)
    WarrantyStartDate = "1900-12-31T23:59:59" (IFCTEXT)
  COBie | properties | on 1 type object
    AccessibilityPerformance = "n/a" (IFCTEXT)
    AssetIdentifier = "n/a" (IFCTEXT)
    AssetType = "Fixed" (IFCTEXT)
    BarCode = "n/a" (IFCTEXT)
    Category = "Pr_25_71_63_15:Compact or solid grade high-pressure laminate (HPL) boards" (IFCTEXT)
    CodePerformance = "n/a" (IFCTEXT)
    Color = "n/a" (IFCTEXT)
    Constituents = "n/a" (IFCTEXT)
    Description = "Duromer high-pressure laminate panels (HPL) in accordance with BS EN 438-6 Type EDF, suitable for long-lasting balconies and façade claddings" (IFCTEXT)
    DurationUnit = "year" (IFCTEXT)
    ExpectedLife = "n/a" (IFCTEXT)
    Features = "Weather-resistant, flame-retardant core, lightfast, double-hardened, scratch and solvent resistant, easy to clean, custom shapes also available" (IFCTEXT)
    Grade = "To BS EN 438-6, Type EDF" (IFCTEXT)
    InstallationDate = "1900-12-31T23:59:59" (IFCTEXT)
    Manufacturer = "office@fundermax.biz" (IFCTEXT)
    ModelNumber = "n/a" (IFCTEXT)
    ModelReference = "Max Exterior F-Quality" (IFCTEXT)
    Name = "CompactOrSolidGradeLaminatesHPL_MaxExteriorFQuality_SP-2800x1850mm_FunderMax" (IFCTEXT)
    NominalHeight = 10. (IFCLENGTHMEASURE) [MILLI METRE]
    NominalLength = 2800. (IFCLENGTHMEASURE) [MILLI METRE]
    NominalWidth = 1850. (IFCLENGTHMEASURE) [MILLI METRE]
    ReplacementCost = "n/a" (IFCTEXT)
    SerialNumber = "n/a" (IFCTEXT)
    Shape = "Rectangle" (IFCTEXT)
    Size = "2800 x 1850 x 10 mm" (IFCTEXT)
    SustainabilityPerformance = "n/a" (IFCTEXT)
    TagNumber = "n/a" (IFCTEXT)
    WarrantyDescription = "n/a" (IFCTEXT)
    WarrantyDurationLabor = "n/a" (IFCTEXT)
    WarrantyDurationParts = "n/a" (IFCTEXT)
    WarrantyDurationUnit = "year" (IFCTEXT)
    WarrantyGuarantorLabor = "n/a" (IFCTEXT)
    WarrantyGuarantorParts = "n/a" (IFCTEXT)
    WarrantyStartDate = "1900-12-31T23:59:59" (IFCTEXT)
  COBie | properties | on 1 type object
    AccessibilityPerformance = "n/a" (IFCTEXT)
    AssetIdentifier = "n/a" (IFCTEXT)
    AssetType = "Fixed" (IFCTEXT)
    BarCode = "n/a" (IFCTEXT)
    Category = "Pr_25_71_63_15:Compact or solid grade high-pressure laminate (HPL) boards" (IFCTEXT)
    CodePerformance = "n/a" (IFCTEXT)
    Color = "n/a" (IFCTEXT)
    Constituents = "n/a" (IFCTEXT)
    Description = "Duromer high-pressure laminate panels (HPL) in accordance with BS EN 438-6 Type EDF, suitable for long-lasting balconies and façade claddings" (IFCTEXT)
    DurationUnit = "year" (IFCTEXT)
    ExpectedLife = "n/a" (IFCTEXT)
    Features = "Weather-resistant, flame-retardant core, lightfast, double-hardened, scratch and solvent resistant, easy to clean, custom shapes also available" (IFCTEXT)
    Grade = "To BS EN 438-6, Type EDF" (IFCTEXT)
    InstallationDate = "1900-12-31T23:59:59" (IFCTEXT)
    Manufacturer = "office@fundermax.biz" (IFCTEXT)
    ModelNumber = "n/a" (IFCTEXT)
    ModelReference = "Max Exterior F-Quality" (IFCTEXT)
    Name = "CompactOrSolidGradeLaminatesHPL_MaxExteriorFQuality_JU-4100x1300mm_FunderMax" (IFCTEXT)
    NominalHeight = 10. (IFCLENGTHMEASURE) [MILLI METRE]
    NominalLength = 4100. (IFCLENGTHMEASURE) [MILLI METRE]
    NominalWidth = 1300. (IFCLENGTHMEASURE) [MILLI METRE]
    ReplacementCost = "n/a" (IFCTEXT)
    SerialNumber = "n/a" (IFCTEXT)
    Shape = "Rectangle" (IFCTEXT)
    Size = "4100 x 1300 x 10 mm" (IFCTEXT)
    SustainabilityPerformance = "n/a" (IFCTEXT)
    TagNumber = "n/a" (IFCTEXT)
    WarrantyDescription = "n/a" (IFCTEXT)
    WarrantyDurationLabor = "n/a" (IFCTEXT)
    WarrantyDurationParts = "n/a" (IFCTEXT)
    WarrantyDurationUnit = "year" (IFCTEXT)
    WarrantyGuarantorLabor = "n/a" (IFCTEXT)
    WarrantyGuarantorParts = "n/a" (IFCTEXT)
    WarrantyStartDate = "1900-12-31T23:59:59" (IFCTEXT)
  COBie | properties | on 1 type object
    AccessibilityPerformance = "n/a" (IFCTEXT)
    AssetIdentifier = "n/a" (IFCTEXT)
    AssetType = "Fixed" (IFCTEXT)
    BarCode = "n/a" (IFCTEXT)
    Category = "Pr_25_71_63_15:Compact or solid grade high-pressure laminate (HPL) boards" (IFCTEXT)
    CodePerformance = "n/a" (IFCTEXT)
    Color = "n/a" (IFCTEXT)
    Constituents = "n/a" (IFCTEXT)
    Description = "Duromer high-pressure laminate panels (HPL) in accordance with BS EN 438-6 Type EDF, suitable for long-lasting balconies and façade claddings" (IFCTEXT)
    DurationUnit = "year" (IFCTEXT)
    ExpectedLife = "n/a" (IFCTEXT)
    Features = "Weather-resistant, flame-retardant core, lightfast, double-hardened, scratch and solvent resistant, easy to clean, custom shapes also available" (IFCTEXT)
    Grade = "To BS EN 438-6, Type EDF" (IFCTEXT)
    InstallationDate = "1900-12-31T23:59:59" (IFCTEXT)
    Manufacturer = "office@fundermax.biz" (IFCTEXT)
    ModelNumber = "n/a" (IFCTEXT)
    ModelReference = "Max Exterior F-Quality" (IFCTEXT)
    Name = "CompactOrSolidGradeLaminatesHPL_MaxExteriorFQuality_XL-4100x1850mm_FunderMax" (IFCTEXT)
    NominalHeight = 10. (IFCLENGTHMEASURE) [MILLI METRE]
    NominalLength = 4100. (IFCLENGTHMEASURE) [MILLI METRE]
    NominalWidth = 1850. (IFCLENGTHMEASURE) [MILLI METRE]
    ReplacementCost = "n/a" (IFCTEXT)
    SerialNumber = "n/a" (IFCTEXT)
    Shape = "Rectangle" (IFCTEXT)
    Size = "4100 x 1850 x 10 mm" (IFCTEXT)
    SustainabilityPerformance = "n/a" (IFCTEXT)
    TagNumber = "n/a" (IFCTEXT)
    WarrantyDescription = "n/a" (IFCTEXT)
    WarrantyDurationLabor = "n/a" (IFCTEXT)
    WarrantyDurationParts = "n/a" (IFCTEXT)
    WarrantyDurationUnit = "year" (IFCTEXT)
    WarrantyGuarantorLabor = "n/a" (IFCTEXT)
    WarrantyGuarantorParts = "n/a" (IFCTEXT)
    WarrantyStartDate = "1900-12-31T23:59:59" (IFCTEXT)
  IFC | properties | on 4 type objects